[image: ]
Data Sheet

	KEN Washer Disinfector IQ3


	
	Standard Range Features

· OLED Display with soft touch program keys on control panel
· Open Programs Structure
· Very low water consumption
· Low Noise Levels
· Low Energy Costs
· Maintenance free sliding doors
· Service access from the front
· EN ISO 15883-1-2-5-6 compliant
· Glass surfaces easy to clean
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	IQ3

	Outer dimensions
Outer dimensions with side cabinet
	H: 840 x W: 600 x D: 630 mm
H: 840 x W: 900 x D: 630 mm

	Wash chamber dimensions
	H: 490 x W: 540 x D: 556 mm

	Operative volume, wash chamber
	150 Litres

	Total chamber volume
	170 Litres

	Capacity of DIN baskets (480x250x50mm)  
	4x2 DIN Baskets

	Water consumption per phase (4 level rack)
	8-14 litres

	Programs
	10 Standard + 30 optional

	Process times
	Standard 40-60 min. 

	Water connection
	1 x ¾” (2 x ¾” are optional)

	Cold water Pressure
	2-8 Bar, ≥15L/min, 5-30˚, 0-30˚dH

	Hot water
	2-8 Bar, ≥15L/min, 30-70˚, 0-3˚dH

	Demineralised/RO water
	2-8 Bar, 15L/min 5-70˚ cond. 0-200μS

	Condenser
	Standard


							
							
* The above is the standard specification. Any modification/deviation for the above will be clearly identified on the quotation front sheet.


Additional Options and Accessories:			XML server Connection
							Printer
							2 x Additional Water Connections
							Drying Module
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Leading specialists in laboratory and medical
sterilization and decontamination solutions.
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